(Your Business Name Here) – Safe Work Procedure
INJECTION MOULDER

DO NOT use this machine unless you have been instructed
in its safe use and operation and have been given permission

PERSONAL PROTECTIVE EQUIPMENT
	[image: Safety glasses must be warn at all times in work areas]Safety glasses must be worn at all times in work areas.

	[image: Long and loose hair must be contained]Long and loose hair must be contained.
	[image: Gloves must be worn]Gloves must be worn.

	[image: Sturdy footwear must be worn at all times in work areas]Sturdy footwear must be worn at all times in work areas.
	[image: Close fitting/protective clothing must be worn]Close fitting/protective clothing must be worn.
	[image: Rings and jewellery must not be worn]Rings and jewellery must not be worn.




PRE-OPERATIONAL SAFETY CHECKS
[bookmark: OLE_LINK19][bookmark: OLE_LINK20]Locate and ensure you are familiar with all machine operations and controls.
[bookmark: OLE_LINK27][bookmark: OLE_LINK29][bookmark: OLE_LINK31][bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK24][bookmark: OLE_LINK25][bookmark: OLE_LINK16][bookmark: OLE_LINK17]Ensure all guards are fitted, secure and functional. Do not operate if guards are missing or faulty.
Check workspaces and walkways to ensure no slip/trip hazards are present. 

OPERATIONAL SAFETY CHECKS
Keep clear of moving machine parts.
Be aware of other people in the area.  
Pre-heat the injection moulder to be sure the machine has reached the required temperature.

ENDING OPERATIONS AND CLEANING UP
Switch off the machine when work completed.
Before making adjustments or before cleaning material accumulations, switch off and bring the machine to a complete standstill. 
Leave the machine and work area in a safe, clean and tidy state.

POTENTIAL HAZARDS AND INJURIES
Crush points.
Hot machinery parts	.
[bookmark: OLE_LINK8][bookmark: OLE_LINK9][bookmark: OLE_LINK13][bookmark: OLE_LINK18][bookmark: OLE_LINK21][bookmark: OLE_LINK26][bookmark: OLE_LINK30]Hair/clothing getting caught in moving machine parts.
Eye injuries.

DON’T
Do not use faulty equipment. Immediately report suspect machinery. 
Never leave the machine running unattended.  









































This safe work procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with other references. 
It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use.

ALWAYS refer to the manufacturer’s instructions when writing your own safe work procedure.
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