(Your Business Name Here) Safe Work Procedure
BELT DISC SANDER

DO NOT use this machine unless you have been instructed
in its safe use and operation and have been given permission

PERSONAL PROTECTIVE EQUIPMENT


	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - EYE  PROTECTION MUST BE WORN]Safety glasses must be worn at all times in work areas.

	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - LONG & LOOSE HAIR MUST BE CONTAINED]Long and loose hair must be contained.
	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - GLOVES MUST NOT BE WORN]Gloves must not be worn.

	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - FOOT PROTECTION MUST BE WORN]Sturdy footwear must be worn at all times in work areas.
	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN - Close fitting/protective clothing must be worn]Close fitting/protective clothing must be worn.
	[image: PERSONAL PROTECTIVE EQUIPMENT SIGN  RING & JEWELLERY MUST NOT BE WORN][image: ]Rings and jewellery must not be worn.




PRE-OPERATIONAL SAFETY CHECKS
[bookmark: OLE_LINK19][bookmark: OLE_LINK20][bookmark: OLE_LINK34]Locate and ensure you are familiar with all machine operations and controls. 
[bookmark: OLE_LINK4][bookmark: OLE_LINK5][bookmark: OLE_LINK6][bookmark: OLE_LINK7][bookmark: OLE_LINK12][bookmark: OLE_LINK27][bookmark: OLE_LINK28][bookmark: OLE_LINK29][bookmark: OLE_LINK31][bookmark: OLE_LINK37][bookmark: OLE_LINK38][bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK24][bookmark: OLE_LINK25][bookmark: OLE_LINK16][bookmark: OLE_LINK17]Ensure all guards are fitted, secure and functional. Do not operate if guards are missing or faulty.
Check workspaces and walkways to ensure no slip/trip hazards are present.
Ensure the table is set not more than 2mm from disc.
Check belts and discs are in a serviceable condition. 
Stand out of the direct line of the abrasive belt at all times.
Start the dust extraction unit before using the machine.

OPERATIONAL SAFETY CHECKS
Only one person may operate this machine at any one time.
Allow machine to reach maximum revolutions before operating to avoid overloading.
Always place material on the table on the downward side of the disc travel to hold it down on the table surface.
Hold material firmly against stops or table before applying pressure on abrasive.
Keep fingers clear of disc or belt while sanding.
Before making adjustments, switch off and bring the machine to a complete standstill. 

ENDING OPERATIONS AND CLEANING UP
Switch off the machine when work completed.
Leave the machine in a safe, clean and tidy state.

POTENTIAL HAZARDS AND INJURIES
Abrasions.
Burns to skin.
Eye injuries.
Excessive dust.
Unsecured material being flung around.


DON’T
Do not use faulty equipment. Immediately report suspect machinery. 
Do not sand very small items.
Do not sharpen tools with the sander.
Do not sand metal.
Never leave the machine running attended.





























This safe work procedure does not necessarily cover all possible hazards associated with this equipment and should be used in conjunction with other references. 
It is designed as a guide to be used to compliment training and as a reminder to users prior to equipment use.

ALWAYS refer to the manufacturer’s instructions when writing your own safe work procedure.
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